For 1990-2009 cars

#### Fastener Tightening Specifications

Description of Usage | Ref. No.* | Qty | Size | Specification
--- | --- | --- | --- | ---
Metric | English
2-1 Servo to Case | 103 | 3 | M8x1.25x25 | 25 N·m | 18 lb ft
Accumulator Cover to Case | 131 | 11 | M6x1.0x28 | 12 N·m | 106 lb in
Case Cover to Case | 434 | 3 | M6x1.0x40 | 12 N·m | 106 lb in
Case Cover to Case | 436 | 3 | M6x1.0x30 | 12 N·m | 106 lb in
Case Cover to Driven Sprocket Support | 435 | 3 | M8x1.25x50 | 25 N·m | 18 lb ft
Case Cover to Driven Sprocket Support (TORX®) | 433 | 1 | M6x1.0x32 | 12 N·m | 106 lb in
Case to Drive Sprocket Support | 524 | 4 | M8x1.25x23 | 25 N·m | 18 lb ft
Case Extension to Case | 5 | 4 | M10x1.5x35 | 36 N·m | 26 lb ft
Case Side Cover to Case | 56 | 9 | M8x1.25x25 | 25 N·m | 18 lb ft
Case Side Cover to Case (Stud) | 58 | 4 | M8x1.25x25 | 25 N·m | 18 lb ft
Case Side Cover to Case (TORX® Special) | 57 | 4 | M8x1.25x21 | 25 N·m | 18 lb ft
Detent Spring to Case Cover | 805 | 1 | M6x1.0x16 | 12 N·m | 106 lb in
Forward Band Servo Cover to Case | 12 | 3 | M6x1.0x20 | 12 N·m | 106 lb in
Manual Shaft/Detent Nut | 803 | 1 | M10x1.5 | 32 N·m | 23 lb ft
Oil Cooler Quick Connector | 62 | 1 | 1/4-18 NPSF | 38 N·m | 28 lb ft
Oil Cooler Quick Connector with Checkball | 61 | 1 | 3/8-18 NPSF | 38 N·m | 28 lb ft
Oil Pan to Case | 23 | 20 | M6x1.0x18 | 14 N·m | 10 lb ft
Oil Pressure Test Hole Plug | 38 | 1 | 1/8-27 NPTF | 12 N·m | 106 lb in
Pump Body to Case | 206 | 2 | M6x1.0x95 | 16 N·m | 11 lb ft
Pump Cover to Case Cover | 207 | 9 | M6x1.0x85 | 12 N·m | 106 lb in
Pump Cover to Pump Body | 205 | 1 | M6x1.0x20 | 8 N·m | 70 lb in
Speed Sensor to Case | 9 | 1 | M8x1.25x12 | 12 N·m | 106 lb in
TFP Switch to Case | 379 | 1 | M6x1.0x95 | 16 N·m | 11 lb ft
TFP Switch to Case Cover | 375 | 3 | M6x1.0x60 | 12 N·m | 106 lb in
TFP Switch to Valve Body | 381 | 2 | M6x1.0x20 | 8 N·m | 70 lb in
Valve Body to Case | 374 | 3 | M6x1.0x65 | 12 N·m | 106 lb in
Valve Body to Case | 384 | 1 | M6x1.0x85 | 12 N·m | 106 lb in
Valve Body to Case Cover | 376 | 1 | M6x1.0x30 | 12 N·m | 106 lb in
Valve Body to Case Cover | 378 | 3 | M6x1.0x55 | 12 N·m | 106 lb in
Valve Body to Case Cover (TORX®) | 377 | 2 | M6x1.0x45 | 12 N·m | 106 lb in
Valve Body to Driven Sprocket Support | 380 | 1 | M8x1.25x90 | 25 N·m | 18 lb ft
* Reference Number refers to the callout number on the disassembled view.

Description of Usage | Specification
--- | ---
Metric | English
2-1 Servo to Case | 25 N·m | 18 lb ft
Accumulator Cover to Case | 12 N·m | 106 lb in
Case Cover to Case | 12 N·m | 106 lb in
Case Cover to Case | 12 N·m | 106 lb in
Case Cover to Driven Sprocket Support | 25 N·m | 18 lb ft
Case Cover to Driven Sprocket Support (Torx) | 12 N·m | 106 lb in
Case to Drive Sprocket Support | 25 N·m | 18 lb ft
Case Extension to Case | 36 N·m | 26 lb ft
Case Side Cover to Case | 25 N·m | 18 lb ft
Case Side Cover to Case (Stud) | 25 N·m | 18 lb ft
Case Side Cover to Case (Torx Special) | 25 N·m | 18 lb ft
Detent Spring to Case Cover | 12 N·m | 106 lb in
Fluid Filler Tube Bolt | 13 N·m | 115 lb in
Fluid Filler Tube Nut | 13 N·m | 115 lb in
Flywheel to Torque Converter Bolts | 63 N·m | 47 lb ft
Forward Band Servo Cover to Case | 12 N·m | 106 lb in
Manual Shaft/Detent Nut | 32 N·m | 23 lb ft
Oil Cooler Hose Clip Bolt | 25 N·m | 17 lb ft
Oil Cooler Pipe Fitting at Radiator | 45 N·m | 33 lb ft
Oil Cooler Quick Connector | 38 N·m | 28 lb ft
Oil Cooler Quick Connector with Checkball | 38 N·m | 28 lb ft
Oil Pan to Case | 14 N·m | 10 lb ft
Oil Pressure Test Hole Plug | 12 N·m | 106 lb in
PNP Switch Bolts | 25 N·m | 18 lb ft
Pump Body to Case | 16 N·m | 11 lb ft
Pump Cover to Case Cover | 12 N·m | 106 lb in
Pump Cover to Pump Body | 8 N·m | 70 lb in
Speed Sensor to Case | 12 N·m | 106 lb in
Torque Converter Cover Bolts | 10 N·m | 89 lb in
Transaxle Brace Bolts | 43 N·m | 32 lb ft
Transaxle Mount Bracket Bolts | 95 | 70 lb ft
Transaxle Mount Lower Nuts | 47 | 35 lb ft
Transaxle Mount Upper Nuts | 47 | 35 lb ft
Transaxle Range Selector Cable Bracket Bolts | 25 | 18 lb ft
Transaxle to Engine Bolts | 75 | 55 lb ft
Transaxle to Engine Stud | 75 | 55 lb ft
TFP Switch to Case | 16 N·m | 11 lb ft
TFP Switch to Case Cover | 12 N·m | 106 lb in
TFP Switch to Valve Body | 8 N·m | 70 lb in
Valve Body to Case | 12 N·m | 106 lb in
Valve Body to Case | 12 N·m | 106 lb in
Valve Body to Case Cover | 12 N·m | 106 lb in
Valve Body to Case Cover | 12 N·m | 106 lb in
Valve Body to Case Cover (Torx) | 12 N·m | 106 lb in
Valve Body to Driven Sprocket Support | 25 N·m | 18 lb ft
* Reference Number refers to the callout number on the disassembled view.