For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Disconnect the front door wiring harness and electrical connectors.
4. Remove the route wire harness from the front door conduit.
5. Remove the front door conduit from the front door.

### Installation Procedure

1. Install the front door conduit to the front door.
2. Install the route wiring harness to the front door conduit.
3. Connect the front door wiring harness and electrical connectors.
4. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install the front door trim panel. Refer to Door Trim Panel Replacement .