For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the driver seat. Refer to Bucket Seat Replacement in Seats.
3. Remove the driver seat adjuster track cover (1). Refer to Front Seat Adjuster Track Finish Cover Replacement in Seats.
4. Remove the nut from the driver seat belt pretensioner (1) .
5. Route the driver seat belt pretensioner wiring harness (2) through the driver seat bottom frame.
6. Remove the driver seat belt pretensioner (1) from the driver seat bottom frame.
7. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Pretensioner Handling, Shipping, and Scrapping .

### Installation Procedure

1. Install the driver seat belt pretensioner (1) to the driver seat bottom frame.
2. Route the driver seat belt pretensioner wiring harness (2) through the driver seat bottom frame.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the nut to the driver seat belt pretensioner (1).

Tighten
Tighten the nut to 35 N·m (26 lb ft).

4. Install the driver seat adjuster track cover (1). Refer to Front Seat Adjuster Track Finish Cover Replacement in Seats.
5. Install the driver seat. Refer to Bucket Seat Replacement in Seats.
6. Enable the SIR system. Refer to Enabling the SIR System .