For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the front side door window. Refer to Front Side Door Window Replacement .
4. Remove the power window regulator. Refer to Front Side Door Window Regulator Replacement .

1 | Power Window Motor Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Power Window Regulator Motor