For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .

1 | Lower Grille Molding Screws (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Lower Grille Molding Procedure Release the upper retainers from inside the front bumper fascia and remove the grille from the front bumper fascia.