For 1990-2009 cars

Use the urethane adhesive for replacement of any urethane adhesive-installed window using the full cut method.

In the United States or Canada, you may use urethane adhesive systems which meet GM Specification GM 3651G.

Use these materials based on specific manufacturer. Do NOT intermix primers or adhesives from one manufacturer to another.

Always follow the system manufacturer's instructions for application, handling, and curing.