For 1990-2009 cars

#### Tools Required

J 44827 Transmission Cooler Quick Disconnect

### Removal Procedure

1. Locate the transmission oil cooler (TOC) quick connect fitting (1).

Important: Be sure that the lock tang on the release tool is properly engaged.

2. Install the J 44827 onto the TOC pipe.
3. Slide the J 44827 toward the TOC quick connect fitting.
4. Insert the J 44827 into the TOC quick connect fitting. The distance between the quick connect fitting and J 44827 should be approximately 2.00 mm (0.080 in).
5. Pull back on the TOC pipe to disengage the pipe from the TOC quick connect fitting.
6. Remove the J 44827 from the TOC pipe.

### Installation Procedure

Important: Inspect the TOC quick connect fitting for signs of wear or damage. Replace the components if necessary.

1. Install the TOC pipe into the TOC quick connect fitting.

A distinct snap should be heard or felt when assembling the TOC pipe to the quick connect fitting.

2. To ensure the cooler line is properly installed, give the cooler pipe a gentle pull.