For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Power Steering System Description and Operation
2 | Verify that the steering column is loose. Is the steering column loose? | Go to Step 3 | System OK
3 | Inspect the steering column mounting brackets for looseness. Are the steering column mounting brackets loose? | Go to Step 6 | Go to Step 4
4 | Verify that the steering column bracket capsule is not sheared. Is the steering column bracket capsule sheared? | Go to Step 7 | Go to Step 5
5 | Inspect the intermediate shaft for worn joints or looseness. Is the intermediate joint worn or loose? | Go to Step 8 | Go to Step 9
6 | Notice: Refer to Fastener Notice in the Preface section. Tighten the mounting bolts to specifications. Refer to Fastener Tightening Specifications . Did you complete the repair? | Go to Step 9 | --
7 | Replace the steering column assembly. Refer to Steering Column Replacement . Did you complete the replacement? | Go to Step 9 | --
8 | Tighten or replace the intermediate shaft as needed. Refer to Intermediate Steering Shaft Replacement . Did you complete the repair? | Go to Step 9 | --
9 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3