For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the panel. Refer to Front Floor Panel Carpet Filler Replacement .
2. Program the body control module after replacement. Refer to Control Module References .

1 | Body Control Module Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (53 lb in)
2 | Body Control Module Assembly

#### Procedure

Disconnect the electrical connectors.