For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement.
3. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.
4. Remove the generator. Refer to Generator Replacement.
5. Remove the drive belt. Refer to Drive Belt Replacement.

1 | A/C Compressor and Condenser Hose Assembly Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Sealing Washer

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement.

3 | A/C Compressor Bolt (Qty: 3)

#### Procedure

Tighten the bolts in sequence.

Tighten
22 N·m (16 lb ft)

4 | A/C Compressor Assembly