For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the rear compartment lid.
2. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.

1 | Rear Bumper Fascia Center Bracket Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear Bumper Fascia Center Bracket Tip Disconnect the rear license plate electrical harness from the rear bumper fascia bracket prior to removing the bracket.
3 | High Mounted Stop Lamp Screw (Qty: 2) Tighten 2 N·m (18 lb in)
4 | High Mounted Stop Lamp Assembly Procedure Remove the high mounted stop lamp from the rear bumper fascia center bracket.