For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Open the hood.
2. Reach in between the bumper and front hood opening to disconnect the fog lamp electrical connector from the fog lamp socket.

1 | Front Fog Lamp Bulb Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Rotate the bulb socket counterclockwise from the lamp housing in order to remove.