For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector as needed. Refer to Door Water Deflector Replacement .
3. Use a flat-head tool to release the threaded rod (1) from the clip (2).

### Installation Procedure

1. Position the rod in the clip in order to eliminate any free play in the outside door handle.
2. Install the clip cover (2) over the threaded rod (1).
3. Inspect the door lock system for proper operation.
4. Install the water deflector as needed. Refer to Door Water Deflector Replacement .
5. Install the trim panel. Refer to Door Trim Panel Replacement .