For 1990-2009 cars

### Removal Procedure

Caution: Refer to Approved Equipment for Collision Repair Caution in the Preface section.

1. Disable the SIR system. Refer to SIR Disabling and Enabling .
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
3. Remove all related panels and components.
4. Repair as much of the damage as possible to factory specifications.
5. Remove the quarter panel. Refer to Quarter Outer Panel Replacement .

Caution: Refer to Foam Sound Deadeners Caution in the Preface section.

6. Note the location and remove the sealers and anti-corrosion materials from the repair area, as necessary. Refer to Anti-Corrosion Treatment and Repair .

Important: Do not damage any inner panels or reinforcements.

7. Locate and drill out all factory rivets. Note the number and location of rivets for installation of the hinge pillar body reinforcement.
8. Remove the damaged hinge pillar body reinforcement.

### Installation Procedure

1. Position the hinge pillar body reinforcement.
2. Install rivets accordingly.
3. Clean and prepare all surfaces.
4. Apply the sealers and anti-corrosion materials to the repair area, as necessary. Refer to Anti-Corrosion Treatment and Repair .
5. Paint the repair area. Refer to Paint Identification .
6. Install the quarter panel. Refer to Quarter Outer Panel Replacement .
7. Install all related panels and components.
8. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
9. Enable the SIR system. Refer to SIR Disabling and Enabling .