For 1990-2009 cars

### Special Tools

• | J 43653 Flywheel Holding Tool

• | J 45059 Angle Meter

1. Install the flywheel.
2. Install the NEW bolts.
3. Install J 43653 flywheel holding tool in the starter assembly location, engaging the flywheel, in order to prevent crankshaft rotation.

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the flywheel bolts to 53 N·m (39 lb ft), plus 25 degrees, using J 45059 meter .