For 1990-2009 cars

#### Special Tools

• | J 8092 Universal Driver Handle

• | J 44766 Seal Installer

For equivalent regional tools, refer to Special Tools.

1. Assemble J 8092 driver handle onto J 44766 seal installer .

Caution: Install the seal onto the installation tool before installing into the case to prevent damage to the seal.

2. Install the seal (229) onto J 44766 seal installer .

Note: Align the torque converter seal with the bolt holes.

3. Install the NEW seal (229) into the housing.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the NEW seal bolts (228). Tighten the seal bolts to 3.6 N·m (31.86 lb in).
5. Install the NEW input shaft seal (430).