For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the 3 hold down bolts for the underhood electrical center and position aside. Refer to Underhood Electrical Center or Junction Block Replacement.
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.

1 | Air Inlet Housing Nut (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Air Inlet Housing Front Panel Assembly