For 1990-2009 cars

1. Inspect the following components:

• | Inspect the transmission fluid pan for distortion, cracks, or score marks.

• | Inspect the fluid pan bolts for thread damage.

• | Inspect the transmission pan magnet for cracks and tears.

2. Install the transmission fluid filter (59) and fluid filters seals (57) into the case (24).
3. Install the fluid pan magnet (61) onto the fluid pan (62).
4. Install the NEW fluid pan gasket (60) onto the fluid pan (62).
5. Install the fluid pan (62) onto the case.

Notice: Refer to Fastener Notice in the Preface section.

6. Install the fluid pan bolts (65) into the case.

Tighten
Tighten the fluid pan bolts to 11 N·m (8 lb ft).