For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
2. Remove the side radiator air lower baffle and deflector. Refer to Radiator Air Lower Baffle and Deflector Replacement .
3. Remove the radiator upper air baffle and deflector. Refer to Radiator Air Upper Baffle and Deflector Replacement .

1 | Power Steering Gear Outlet Hose Clamp

#### Procedure

Remove as much power steering fluid as possible from the remote power steering fluid reservoir.

2 | Power Steering Gear Outlet Hose
3 | Power Steering Fluid Cooler Hose Clamp
4 | Power Steering Fluid Cooler Hose
5 | Power Steering Fluid Cooler Pipe Bracket Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
6 | Power Steering Fluid Cooler

#### Procedure

1. Remove the power steering fluid cooler from the bottom of the vehicle.
2. Fill and bleed the power steering system. Refer to Power Steering System Bleeding