For 1990-2009 cars

Caution: Refer to Express Down Feature Caution in the Preface section.

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Reconnect the window switch to the harness.
3. Position the window to the full up position.
4. Disconnect the window switch from the harness.
5. Loosen the window clamps.
6. Close the door.
7. With the aid of an assistant standing outside of the vehicle, position the window to the door opening.
8. From the inside of the vehicle tighten the window clamps.
9. Perform minor height and minor tip-in adjustments as necessary. Refer to Door Window Tip-In Adjustment .
10. Install the door trim panel. Refer to Door Trim Panel Replacement .