For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the air deflector. Refer to Front Bumper Fascia Air Deflector Replacement .
3. Remove the energy absorber. Refer to Front Bumper Fascia Energy Absorber Replacement .
4. Remove the front bumper impact bar bracket. Refer to Front Bumper Impact Bar Bracket Replacement .

1 | Front Impact Bar Bolt (Qty: 8) Notice: Refer to Fastener Notice in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Front Impact Bar Bolt (Qty: 4) Tighten 9 N·m (80 lb in)
3 | Front Impact Bar