For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the rear compartment lid buttress latch release cable and pull it through the lid and set it aside with the pass-through grommet. Refer to Rear Compartment Lid Buttress Latch Release Cable Replacement.
2. Before installing the deck lid to the vehicle, apply a 6 mm bead of 3M® 08405 Flex Clear Seam Sealer or equivalent, to the upper interface joint of the seal flange to the deck inner lid (a).

1 | Rear Compartment Lid Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (19 lb ft)
2 | Rear Compartment Lid Tip Transfer any parts over to the new lid if needed.