For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Door Water Deflector Replacement.
3. Remove the front side door window. Refer to Front Side Door Window Replacement.
4. Remove the power window regulator. Refer to Front Side Door Window Regulator Replacement.

1 | Power Window Motor Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Power Window Regulator Motor