For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.

1 | Charge Air Cooler Pipe Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Radiator Upper Bracket Nut (Qty: 2) Tighten 9 N·m (80 lb in)
3 | Charge Air Cooler Pipe Rear Bracket
4 | Air Cleaner Stud Tighten 10 N·m (89 lb in)
5 | Radiator Upper Bracket Assembly