For 1990-2009 cars

### Rear Window Defogger System Components

The rear window defogger system consist of the following components:

• | Body control module (BCM)

• | HVAC control module

• | Rear window defog relay

• | Rear window defogger grid

### Rear Window Defogger Operation

The body control module (BCM) controls the rear window defog relay located in the underhood fuse block. The rear window defog switch located on the HVAC control module is hard wired to the BCM. The rear window defog switch provides the request signal to the BCM. With the ignition switch in the RUN position, the BCM supplies voltage to the rear window defog switch via the rear defog switch signal circuit. When the rear window defog switch is pressed, the switch contacts close and ground is supplied. The BCM interprets the flow of voltage as a request to turn the rear defogger ON. The BCM energizes the rear window defog relay by applying voltage to the relay coil via the rear defog relay control circuit. When the rear window defog relay coil is energized, the switch contacts of the rear window defog relay close allowing battery voltage to flow from the REAR DEFOG fuse through the closed switch contacts and out the relay switched output to the rear window defogger grid. Ground for the rear window defogger grid is provided at G301. The BCM also illuminates the rear defog indicator LED located on the HVAC control module with the supplied voltage from the rear defog relay control circuit.

When you start the engine and depress the rear window defogger switch, the defogger cycle lasts for 15 minutes. Further operation will result in 7.5 minute defogger cycles. The rear window defogger cycle resets to 15 minutes when the ignition is cycled from OFF to ON.

The rear window defogger will not time out if vehicle speed is above 50 mph (80 km/h).