For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .
3. Remove the wiper drive system module. Refer to Windshield Wiper Transmission Replacement .

1 | Windshield Wiper Motor Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 4.5 N·m (40 lb in)
2 | Windshield Wiper Motor Assembly Procedure

1. Use the J 39232 Wiper Linkage Separator, or equivalent to separate the transmission arm from the wiper motor crank arm pivot.
2. Use the J 39529 Wiper Linkage Installer, or equivalent to install the transmission arm onto the wiper motor crank arm pivot.