For 1990-2009 cars

Connector 1: | X100 Engine Harness to the I/P Body Harness
Connector 2: | X101 Engine Harness to Transmission Harness (M82)
Connector 3: | X102 Right Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness
Connector 4: | X103 Left Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness
Connector 5: | X110 Forward Lamp Harness to Left Headlamp Assembly Harness
Connector 6: | X111 Forward Lamp Harness to Right Headlamp Assembly Harness
Connector 7: | X120 Instrument Panel Body Harness to the Forward Lamp Harness
Connector 8: | X122 Forward Lamp Harness to the Outside Air Temperature Sensor Harness
Connector 9: | X162 Engine Harness to the Fuel Injector Jumper Harness (LNF)
Connector 10: | X207 Instrument Panel Body Harness to the Console Harness (M82)
Connector 11: | X208 SIR I/P Module Harness to the I/P Body Harness
Connector 12: | X216 I/P Body Harness to the HVAC Harness
Connector 13: | X218 I/P Body Harness to the HVAC Harness
Connector 14: | X316 I/P Body Harness to the Passenger Seat Harness
Connector 15: | X317 I/P Body Harness to the Driver Seat Harness (AF2)
Connector 16: | X317 I/P Body Harness to the Driver Seat Harness (without AF2)
Connector 17: | X400 I/P Body Harness to the Rear Lamp Harness
Connector 18: | X405 Rear Chassis Harness to Left Rear Lamp Assembly Harness
Connector 19: | X406 I/P Body Harness to Chassis Harness
Connector 20: | X407 Rear Chassis Harness to Right Rear Lamp Assembly Harness
Connector 21: | X408 Chassis Harness to I/P Body Harness
Connector 22: | X409 Chassis Harness to I/P Body Harness
Connector 23: | X410 I/P Body Harness to the Rear Lamp Jumper Harness
Connector 24: | X500 Driver Door Harness to the I/P Body Harness
Connector 25: | X501 Driver Door Harness to the I/P Body Harness (A31)
Connector 26: | X505 Driver Door Harness to Power Mirror Switch Harness
Connector 27: | X600 Passenger Door Harness to the Instrument Panel Body Harness

### X100 Engine Harness to the I/P Body Harness

#### Connector Part Information

- OEM: 15443822
- Service: See Catalog
- Description: 40-Way F GT 150 280 Series Sealed 4.0 5.2 (BK)

#### Connector Part Information

- OEM: 15317380
- Service: See Catalog
- Description: 40-Way F GT 150 280 Series Sealed (BK)

#### Terminal Part Information

- Pins: A1-A3, A8, B1-B3, B5, B8-B12, C1-C5, D1, D6, D7
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: C6, C7, B6, A4, A5, B7
- Terminal/Tray: 15304716/8
- Core/Insulation Crimp: Pins: C6, C7 : E/1
- Core/Insulation Crimp: Pins: B6 : See Terminal Repair Kit
- Core/Insulation Crimp: Pins: A4, A5, B7 : 2/1
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A1-A5, A8, B1-B3, B5-B12, C1-C7, D1, D6, D7
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X100 Engine Harness to the I/P Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.5 WH | 1310 | Evaporative Emission (EVAP) Canister Vent Solenoid Control | A1 | 0.5 WH | 1310 | Evaporative Emission (EVAP) Canister Vent Solenoid Control
A2 | 0.5 RD/WH | 840 | Battery Positive Voltage | A2 | 0.5 RD/WH | 840 | Battery Positive Voltage
A3 | 0.35 TN | 1274 | 5-Volt Reference 3 | A3 | 0.35 TN | 1274 | 5-Volt Reference 3
A4 | 1.0 PU | 92 | Windshield Wiper Motor High Speed | A4 | 1.0 PU | 92 | Windshield Wiper Motor High Speed
A5 | 1.0 D-GN | 95 | Windshield Washer Switch Signal | A5 | 1.0 D-GN | 95 | Windshield Washer Switch Signal
A6-A7 | -- | -- | Not Used | A6-A7 | -- | -- | Not Used
A8 | 0.35 BN | 4 | Accessory Voltage | A8 | 0.35 BN | 4 | Accessory Voltage
B1 | 0.35 BN/WH | 419 | MIL Control | B1 | 0.35 BN/WH | 419 | MIL Control
B2 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+) | B2 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
B3 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-) | B3 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
B4 | -- | -- | Not Used | B4 | -- | -- | Not Used
B5 | 0.5 RD/WH | 840 | Battery Positive Voltage | B5 | 0.5 RD/WH | 840 | Battery Positive Voltage
B6 | 0.35 PU | 1272 | Low Reference | B6 | 0.35 PU | 1272 | Low Reference
B7 | 1.0 BK | 250 | Ground | B7 | 1.0 BK | 250 | Ground
B8 | 0.35 L-BU | 1162 | Accelerator Pedal Position Sensor 2 Signal | B8 | 0.35 L-BU | 1162 | Accelerator Pedal Position Sensor 2 Signal
B9 | 0.35 WH/BK | 1164 | 5-Volt Reference 2 | B9 | 0.35 WH/BK | 1164 | 5-Volt Reference 2
B10 | 0.35 BN | 1271 | Low Reference | B10 | 0.35 BN | 1271 | Low Reference
B11 | 0.35 D-BU | 1161 | Adjustable Accelerator Pedal Position (APP) Sensor 1 Signal | B11 | 0.35 D-BU | 1161 | Adjustable Accelerator Pedal Position (APP) Sensor 1 Signal
B12 | 0.5 TN | 2759 | Low Reference | B12 | 0.5 TN | 2759 | Low Reference
C1 | 0.5 PU | 1589 | Fuel Level Sensor Signal | C1 | 0.5 PU | 1589 | Fuel Level Sensor Signal
C2 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal | C2 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
C3 | 0.5 GY | 2709 | 5-Volt Reference 1 | C3 | 0.5 GY | 2709 | 5-Volt Reference 1
C4 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control | C4 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control
C5 | 0.5 YE | 196 | Windshield Wiper Motor Park Switch Signal | C5 | 0.5 YE | 196 | Windshield Wiper Motor Park Switch Signal
C6 | 0.5 PK/BK | 5291 | Ignition 1 Voltage | C6 | 0.5 PK/BK | 5291 | Ignition 1 Voltage
C7 | 0.5 PK | 849 | Brake Fluid Level Sensor Signal | C7 | 0.5 PK | 849 | Brake Fluid Level Sensor Signal
C8-C12 | -- | -- | Not Used | C8-C12 | -- | -- | Not Used
D1-D3 | -- | -- | Not Used | D1-D3 | -- | -- | Not Used
D4-D5 | -- | -- | Not Available | D4-D5 | -- | -- | Not Available
D6 | 0.5 L-GN | 1478 | Coolant Level Switch Signal | D6 | 0.5 L-GN | 1478 | Coolant Level Switch Signal
D7 | 0.5 OG | 228 | Windshield Washer Pump Control | D7 | 0.5 OG | 228 | Windshield Washer Pump Control
D8 | -- | -- | Not Used | D8 | -- | -- | Not Used

### X101 Engine Harness to Transmission Harness (M82)

#### Connector Part Information

- OEM: 9432021
- Service: See Catalog
- Description: 20-Way F (BK) Locking

#### Connector Part Information

- OEM: 96042847
- Service: See Catalog
- Description: Tab Pin Housing 20-Way M (BK) with O-rings

#### X101 Engine Harness to Transmission Harness (M82)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 YE | 400 | Vehicle Speed Signal High Signal | 1 | 0.35 OG | 400 | Vehicle Speed Signal High Signal
2 | 0.35 OG/BK | 1786 | Ignition Lock Cylinder Control Actuator Signal | 2 | 0.35 BN | 1786 | Ignition Lock Cylinder Control Actuator Signal
3 | 0.35 PU | 401 | Vehicle Speed Signal Low Signal | 3 | 0.35 WH | 401 | Vehicle Speed Signal Low Signal
4 | 0.5 BK/WH | 451 | Ground | 4 | 0.35 GN | 451 | Ground
5 | 0.35 PU | 898 | Shift Solenoid Valve 3 High Control | 5 | 0.35 GY | 898 | Shift Solenoid Valve 3 High Control
6 | 0.35 TN | 2762 | Low Reference | 6 | 0.35 WH | 2762 | Low Reference
7 | 0.35 YE | 772 | Transmission Range Switch Signal B | 7 | 0.35 BK | 772 | Transmission Range Switch Signal B
8 | 0.35 L-BU/WH | 1229 | Pressure Control Solenoid Valve Low Control | 8 | 0.35 WH | 1229 | Pressure Control Solenoid Valve Low Control
9 | 0.35 YE/BK | 1223 | 2-3 Shift Solenoid Valve Control | 9 | 0.35 BU | 1223 | 2-3 Shift Solenoid Valve Control
10 | 0.35 YE/BK | 1227 | Transmission Temperature Sensor Signal | 10 | 0.35 RD | 1227 | Transmission Temperature Sensor Signal
11 | 0.35 WH | 776 | Transmission Range Switch Signal P | 11 | 0.35 GY | 776 | Transmission Range Switch Signal P
12 | -- | -- | Not Used | 12 | -- | -- | Not Used
13 | 0.35 OG/BK | 1228 | Pressure Control Solenoid Valve High Control | 13 | 0.35 GN | 1228 | Pressure Control Solenoid Valve High Control
14 | 0.35 L-GN | 1222 | 1-2 Shift Solenoid Valve Control | 14 | 0.35 BK | 1222 | 1-2 Shift Solenoid Valve Control
15 | 0.35 D-BU/WH | 1231 | Automatic Transmission Input Speed Sensor Low Signal | 15 | 0.35 WH | 1231 | Automatic Transmission Input Speed Sensor Low Signal
16 | 0.35 TN/WH | 771 | Transmission Range Switch Signal A | 16 | 0.35 RD | 771 | Transmission Range Switch Signal A
17 | 0.8 OG | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control | 17 | 0.8 WH | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control
18 | 0.35 OG/BK | 1230 | Automatic Transmission Input Speed Sensor High Signal | 18 | 0.35 YE | 1230 | Automatic Transmission Input Speed Sensor High Signal
19 | 0.35 GY | 773 | Transmission Range Switch Signal C | 19 | 0.35 BU | 773 | Transmission Range Switch Signal C
20 | 0.35 BN | 418 | Torque Convertor Clutch PWM Solenoid Valve Control | 20 | 0.35 YE | 418 | Torque Convertor Clutch PWM Solenoid Valve Control

### X102 Right Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 12186568
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12186271
- Service: 15306054
- Description: 4-Way M Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### X102 Right Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-BU | 15 | Right Turn Signal Lamp Supply Voltage | A | 0.5 D-BU | 15 | Right Turn Signal Lamp Supply Voltage
B | -- | -- | Not Used | B | 0.5 BN | 9 | Not Used
C | 0.8 PU | 2234 | Front Fog Lamp Supply Voltage | C | 0.8 PU | 2234 | Front Fog Lamp Supply Voltage
D | 0.8 BK | 250 | Ground | D | 0.8 BK | 250 | Ground

### X103 Left Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 12186568
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12186271
- Service: 15306054
- Description: 4-Way M Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### X103 Left Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-BU | 14 | Left Turn Signal Lamp Supply Voltage | A | 0.5 L-BU | 14 | Left Turn Signal Lamp Supply Voltage
B | -- | -- | Not Used | B | 0.5 BN | 9 | Not Used
C | 0.8 PU | 2234 | Front Fog Lamp Supply Voltage | C | 0.8 PU | 2234 | Front Fog Lamp Supply Voltage
D | 0.8 BK | 150 | Ground | D | 0.8 BK | 150 | Ground

### X110 Forward Lamp Harness to Left Headlamp Assembly Harness

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15369319
- Service: See Catalog
- Description: 4-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### X110 Forward Lamp Harness to Left Headlamp Assembly Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 OG/WH | 711 | Left Headlamp High Beam Supply Voltage | A | 0.8 BK | -- | Left Headlamp High Beam Supply Voltage
B | 0.8 BK | 150 | Ground | B | 0.8 BK | -- | Ground
C | 0.8 YE | 712 | Left Headlamp Low Beam Supply Voltage | C | 0.8 RD | -- | Left Headlamp Low Beam Supply Voltage
D | 0.8 BK | 150 | Ground | D | 0.8 BK | -- | Ground

### X111 Forward Lamp Harness to Right Headlamp Assembly Harness

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15369319
- Service: See Catalog
- Description: 4-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### X111 Forward Lamp Harness to Right Headlamp Assembly Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage | A | 0.8 BK | -- | Right Headlamp High Beam Supply Voltage
B | 0.8 BK | 250 | Ground | B | 0.8 BK | -- | Ground
C | 0.8 TN/WH | 312 | Right Headlamp Low Beam Supply Voltage | C | 0.8 RD | -- | Right Headlamp Low Beam Supply Voltage
D | 0.8 BK2 | 250 | Ground | D | 0.8 BK | -- | Ground

### X120 Instrument Panel Body Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 15326084
- Service: 15306348
- Description: 16-Way F GT 150 280 Series Sealed 4.0 5.8 (BK)

#### Connector Part Information

- OEM: 15326085
- Service: 15306122
- Description: 16-Way M GT 150 280 Series Sealed 4.0 5.8 (BK)

#### Terminal Part Information

- Pins: A, B, C, D, E, F, G, H, J, K, L, M, N, P, R, S
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A, B, C, D, E, F, G, H, J, K, L, M, N, P, R, S
- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X120 Instrument Panel Body Harness to the Forward Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 PK/BK | 6434 | Can Bus High Serial Data | A | 0.5 PK/BK | 6434 | Can Bus High Serial Data
B | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal | B | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal
C | 0.5 OG | 885 | Low Reference | C | 0.5 OG | 885 | Low Reference
D | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal | D | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
E | 0.5 WH | 883 | Low Reference | E | 0.5 WH | 883 | Low Reference
F | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+) | F | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
G | 0.5 TN | 2501 | High Speed GMLAN Serial Data (-) | G | 0.5 TN | 2501 | High Speed GMLAN Serial Data (-)
H | 0.5 D-GN | 2087 | Combined Vehicle Inertial Sensor Supply Voltage | H | 0.5 D-GN | 2087 | Combined Vehicle Inertial Sensor Supply Voltage
J | 0.5 L-BU | 2088 | Low Reference | J | 0.5 L-BU | 2088 | Low Reference
K | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+) | K | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
L | 0.5 TN | 2501 | High Speed GMLAN Serial Data (-) | L | 0.5 TN | 2501 | High Speed GMLAN Serial Data (-)
M | 0.5 YE/BK | 2160 | Front End Discriminating Sensor Signal | M | 0.5 YE/BK | 2160 | Front End Discriminating Sensor Signal
N | 0.5 GY | 5600 | Low Reference | N | 0.5 GY | 5600 | Low Reference
P | 0.5 YE | 1834 | Forward Discriminating Sensor Signal | P | 0.5 YE | 1834 | Forward Discriminating Sensor Signal
R | 0.5 TN/OG | 5045 | Low Reference | R | 0.5 TN/OG | 5045 | Low Reference
S | 0.5 GY/BK | 6435 | Can Bus Low Serial Data | S | 0.5 GY/BK | 6435 | Can Bus Low Serial Data

### X122 Forward Lamp Harness to the Outside Air Temperature Sensor Harness

#### Connector Part Information

- OEM: 12052641
- Service: 12052641
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12162000
- Service: 12167120
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X122 Forward Lamp Harness to the Outside Air Temperature Sensor Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal | A | 0.5 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal
B | 0.5 YE | 61 | Low Reference | B | 0.5 YE | 61 | Low Reference

### X162 Engine Harness to the Fuel Injector Jumper Harness (LNF)

#### Connector Part Information

- OEM: 33472-1216
- Service: See Catalog
- Description: 12-Way F

#### Connector Part Information

- OEM: 33482-1206
- Service: See Catalog
- Description: 12-Way M

#### Terminal Part Information

- Pins: See Terminal Repair Kit
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X162 Engine Harness to the Fuel Injector Jumper Harness (LNF)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.0 BN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1 | 1 | 1.0 TN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
2 | 1.0 D-BU | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2 | 2 | 1.0 TN | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
3 | 1.0 D-GN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3 | 3 | 1.0 TN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
4 | 1.0 L-BU | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4 | 4 | 1.0 TN | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
5 | 0.5 TN | 808 | Low Reference | 5 | 0.5 GY | 808 | Low Reference
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | 1.0 BN/WH | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1 | 7 | 1.0 TN | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1
8 | 1.0 D-BU | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2 | 8 | 1.0 TN | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2
9 | 1.0 D-GN/WH | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3 | 9 | 1.0 TN | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3
10 | 1.0 L-BU/WH | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4 | 10 | 1.0 TN | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4
11 | 0.5 GY | 598 | 5-Volt Reference | 11 | 0.5 GY | 598 | 5-Volt Reference
12 | 0.5 YE | 2918 | Fuel Rail Pressure Sensor Signal | 12 | 0.5 GY | 2918 | Fuel Rail Pressure Sensor Signal

### X207 Instrument Panel Body Harness to the Console Harness (M82)

#### Connector Part Information

- OEM: E-3581-001
- Service: See Catalog
- Description: 12-Way F 1.5 Series (NA)

#### Connector Part Information

- OEM: E-3584-003
- Service: 88988763
- Description: 12-Way M 1.5 Series (NA)

#### Terminal Part Information

- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X207 Instrument Panel Body Harness to the Console Harness (M82)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 L-GN/WH | 5984 | PRNDL Signal D | 1 | 0.35 L-GN/WH | 5984 | PRNDL Signal D
2 | 0.35 OG/BK | 5983 | PRNDL Signal C | 2 | 0.35 OG/BK | 5983 | PRNDL Signal C
3 | 0.35 PK/BK | 5982 | PRNDL Signal B | 3 | 0.35 PK/BK | 5982 | PRNDL Signal B
4 | 0.35 PU/WH | 5981 | PRNDL Signal A | 4 | 0.35 PU/WH | 5981 | PRNDL Signal A
5 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage | 5 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
6 | 0.35 BN | 4 | Accessory Voltage | 6 | 0.35 BN | 4 | Accessory Voltage
7 | 0.35 D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage | 7 | 0.35 D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage
8 | 0.35 BK/WH | 651 | Ground | 8 | 0.35 BK/WH | 651 | Ground
9 | 0.35 BN | 550 | Ground | 9 | 0.35 BK | 550 | Ground
10 | 0.5 BU | 1932 | Ignition Lock Cylinder Control Actuator Signal | 10 | 0.5 D-GN/WH | 1932 | Ignition Lock Cylinder Control Actuator Signal
11-12 | -- | -- | Not Used | 11-12 | -- | -- | Not Used

### X208 SIR I/P Module Harness to the I/P Body Harness

#### Connector Part Information

- OEM: 15336479
- Service: 88988600
- Description: 4-Way F Metri-Pack 280 (YE)

#### Connector Part Information

- OEM: 15336476
- Service: 15306363
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp:See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X208 SIR I/P Module Harness to the I/P Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.5 PK/BK | 3024 | I/P Module - Stage 1 - Low Control | A1 | 0.5 OG | 3024 | I/P Module - Stage 1 - Low Control
A2 | 0.5 YE | 3025 | I/P Module - Stage 1 - High Control | A2 | 0.5 YE | 3025 | I/P Module - Stage 1 - High Control
B1 | 0.5 L-GN/RD | 3026 | I/P Module - Stage 2 - Low Control | B1 | 0.5 PU | 3026 | I/P Module - Stage 2 - Low Control
B2 | 0.5 RD/WH | 3027 | I/P Module - Stage 2 - High Control | B2 | 0.5 GY | 3027 | I/P Module - Stage 2 - High Control

### X216 I/P Body Harness to the HVAC Harness

#### Connector Part Information

- OEM: 6098-4787
- Service: See Catalog
- Description: 8-Way F 2.8 Series (NA)

#### Connector Part Information

- OEM: 6098-4905
- Service: 88988651
- Description: 8-Way M 2.8 Series (NA)

#### Terminal Part Information

- Pins: 1-6
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: Pins: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 1-6
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X216 I/P Body Harness to the HVAC Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2.0 YE | 60 | Blower Motor Low Control | 1 | 2.0 YE | 60 | Blower Motor Low Control
2 | 2.0 TN | 63 | Blower Motor Medium 1 Control | 2 | 2.0 TN | 63 | Blower Motor Medium 1 Control
3 | 2.0 L-BU | 72 | Medium 2 Blower Motor Control | 3 | 2.0 L-BU | 72 | Medium 2 Blower Motor Control
4 | 3.0 OG | 52 | Blower Motor High Control | 4 | 3.0 OG | 52 | Blower Motor High Control
5 | 3.0 BN | 141 | Ignition 3 Voltage | 5 | 3.0 BN | 141 | Ignition 3 Voltage
6 | 3.0 BK | 550 | Ground | 6 | 3.0 BK | 2050 | Ground
7-8 | -- | -- | Not Used | 7-8 | -- | -- | Not Used

### X218 I/P Body Harness to the HVAC Harness

#### Connector Part Information

- OEM: 15193800
- Service: 15193800
- Description: 12-Way F (NA)

#### Connector Part Information

- OEM: 6098-4900
- Service: 15193797
- Description: 12-Way M (NA)

#### Terminal Part Information

- Pins: 1-12
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X218 I/P Body Harness to the HVAC Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 TN/BK | 2274 | Recirculation Door Control Circuit | 1 | 0.35 TN/BK | 2274 | Recirculation Door Control Circuit
2 | 0.35 D-GN | 1614 | Recirculation Door Control | 2 | 0.35 D-GN | 1614 | Recirculation Door Control
3 | 0.35 D-BU | 1646 | Air Temperature Door Position Signal | 3 | 0.35 D-BU | 1646 | Air Temperature Door Position Signal
4 | 0.35 L-GN | 2275 | Mode Door Position Signal | 4 | 0.35 L-GN | 2275 | Mode Door Position Signal
5 | 0.35 L-GN/BK | 1647 | Recirculation Door Control B | 5 | 0.35 TN/BK | 1647 | Recirculation Door Control B
6 | 0.35 L-BU/BK | 1688 | 5-Volt Reference | 6 | 0.35 L-BU/BK | 1688 | 5-Volt Reference
7 | 0.35 L-GN/BK | 2276 | Defrost Door Position Signal | 7 | 0.35 L-GN/BK | 2276 | Defrost Door Position Signal
8 | 0.35 TN | 2273 | Mode Door Control | 8 | 0.35 TN | 2273 | Mode Door Control
9 | 0.35 D-BU | 1199 | Air Temperature Door Control | 9 | 0.35 D-BU | 1199 | Air Temperature Door Control
10 | 0.35 L-BU | 733 | Air Temperature Door Position Signal | 10 | 0.35 L-BU | 733 | Air Temperature Door Position Signal
11 | 0.35 GY | 6137 | Evaporative Emission Core Temperature Sensor Signal | 11 | 0.35 GY | 6137 | Evaporative Emission Core Temperature Sensor Signal
12 | 0.35 YE | 1791 | Low Reference | 12 | 0.35 YE | 1791 | Low Reference

### X316 I/P Body Harness to the Passenger Seat Harness

#### Connector Part Information

- OEM: 15332145
- Service: 15306407
- Description: 8-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332150
- Service: 88986250
- Description: 8-Way M GT 150 Series (BK)

#### Terminal Part Information

- Pins: A, C, D, E, F, G, H
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A, C, D, E, F, G, H
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X316 I/P Body Harness to the Passenger Seat Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal | A | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal
B | -- | -- | Not Used | B | -- | -- | Not Used
C | 0.35 PK | 5057 | Low Reference | C | 0.35 PK | 5057 | Low Reference
D | 0.35 PK | 353 | I/P Module Suppression Indicator Control | D | 0.35 PK | 353 | I/P Module Suppression Indicator Control
E | 0.35 TN/BK | 723 | I/P Module Disable Switch - Signal | E | 0.35 TN/BK | 723 | I/P Module Disable Switch - Signal
F | 0.35 PK | 1339 | Ignition 1 Voltage | F | 0.35 PK | 1339 | Ignition 1 Voltage
G | 0.35 PK | 5018 | Occupant Sensor Serial Data | G | 0.35 PK | 5018 | Occupant Sensor Serial Data
H | 0.5 BK/WH | 351 | Ground | H | 0.5 BK/WH | 351 | Ground

### X317 I/P Body Harness to the Driver Seat Harness (AF2)

#### Connector Part Information

- OEM: 15326886
- Service: See Catalog
- Description: 4-Way F GT280 (BK)

#### Connector Part Information

- OEM: 15326890
- Service: See Catalog
- Description: 4-Way M GT280 (BK)

#### Terminal Part Information

- Pins: A, C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A, C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X317 I/P Body Harness to the Driver Seat Harness (AF2)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 TN/WH | 238 | Driver Seat Belt Switch Signal | A | 0.35 TN/WH | 238 | Driver Seat Belt Switch Signal
B | 0.35 PK | 5057 | Low Reference | B | 0.35 PK | 5057 | Low Reference
C | 2.0 RD/BK | 642 | Battery Positive Voltage | C | 2.0 RD/BK | 5057 | Battery Positive Voltage
D | 2.0 BK | 550 | Ground | D | 2.0 BK | 550 | Ground

### X317 I/P Body Harness to the Driver Seat Harness (without AF2)

#### Connector Part Information

- OEM: 15332132
- Service: 88953364
- Description: 3-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332133
- Service: 88987881
- Description: 3-Way M GT 150 Series, Unsealed (BK)

#### Terminal Part Information

- Pins: A, C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A, C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X317 I/P Body Harness to the Driver Seat Harness (without AF2)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 TN/WH | 238 | Seat Belt Switch Signal | A | 0.35 TN/WH | 238 | Seat Belt Switch Signal
B | -- | -- | Not Used | B | -- | -- | Not Used
C | 0.35 PK | 5057 | Low Reference | C | 0.35 PK | 5057 | Low Reference

### X400 I/P Body Harness to the Rear Lamp Harness

#### Connector Part Information

- OEM: E-5651-1
- Service: 88988448
- Description: 6-Way F FTS Series, Sealed (D-GY)

#### Connector Part Information

- OEM: E-5655-002
- Service: 88988064
- Description: 6-Way MTS 090 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray:8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: Terminal Repair Kit
- Release Tool/Test Probe: Terminal Repair Kit

#### X400 I/P Body Harness to the Rear Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 BK | 750 | Ground | 1 | 0.8 BK | 750 | Ground
2 | 0.5 BN | 9 | Tail/License Park Lamps Supply Voltage | 2 | 0.5 BN | 9 | Tail/License Park Lamps Supply Voltage
3 | 0.8 L-GN | 24 | Backup Lamp Supply Voltage | 3 | 0.5 L-GN | 24 | Backup Lamp Supply Voltage
4 | 0.8 L-BU | 20 | Stop Lamp Supply Voltage | 4 | 0.5 L-BU | 20 | Stop Lamp Supply Voltage
5 | 0.5 OG | 122 | Rear Fog Lamp Supply Voltage | 5 | 0.5 OG | 122 | Rear Fog Lamp Supply Voltage
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

### X405 Rear Chassis Harness to Left Rear Lamp Assembly Harness

#### Connector Part Information

- OEM: 6189-0319
- Service: 88988448
- Description: 6-Way F TS Series, Sealed (GY)

#### Connector Part Information

- OEM: 6188-0173
- Service: See catalog
- Description: 6-Way M TS 090 Series, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray:8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: Terminal Repair Kit
- Release Tool/Test Probe: Terminal Repair Kit

#### X405 Rear Chassis Harness to Left Rear Lamp Assembly Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 0.8 YE | 618 | Left Rear Turn Signal Lamp Supply Voltage | 2 | 0.8 GN | 618 | Left Rear Turn Signal Lamp Supply Voltage
3 | 0.8 D-BU | 809 | Left Tail Lamp Supply Voltage | 3 | 0.8 RD/BU | 809 | Left Tail Lamp Supply Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 0.8 BK | 1050 | Ground | 5 | 0.8 BK | 1050 | Ground
6 | 0.8 L-BU | 20 | Stop Lamp Supply Voltage | 6 | 0.8 GN/WH | 20 | Stop Lamp Supply Voltage

### X406 I/P Body Harness to Chassis Harness

#### Connector Part Information

- OEM: E-5225-001
- Service: 88988066
- Description: 8-Way F Sealed (BK)

#### Connector Part Information

- OEM: E-5222-003
- Service: 88988067
- Description: 8-Way M (BU)

#### Terminal Part Information

- Pins: 1-3, 6-8
- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 4
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1-3, 6-8
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 4
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X406 I/P Body Harness to Chassis Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 RD/WH | 140 | Battery Positive Voltage | 1 | 0.5 RD/WH | 140 | Battery Positive Voltage
2 | 0.5 WH | 1310 | Evaporative Emission Canister Vent Solenoid Control | 2 | 0.5 WH | 1310 | Evaporative Emission Canister Vent Solenoid Control
3 | 0.5 PU | 1589 | Fuel Level Sensor Signal | 3 | 0.5 PU | 1589 | Fuel Level Sensor Signal
4 | 1.0 GY | 120 | Fuel Pump Supply Voltage | 4 | 1.0 GY | 120 | Fuel Pump Supply Voltage
5 | 1.0 L-BU | 20 | Stop Lamp Supply Voltage | 5 | 1.0 L-BU | 20 | Stop Lamp Supply Voltage
6 | 0.5 TN | 2759 | Low Reference | 6 | 0.5 TN | 2759 | Low Reference
7 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal | 7 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
8 | 0.5 GY | 2709 | 5-Volt Reference 1 | 8 | 0.5 GY | 2709 | 5-Volt Reference 1

### X407 Rear Chassis Harness to Right Rear Lamp Assembly Harness

#### Connector Part Information

- OEM: 6189-0319
- Service: 88988448
- Description: 6-Way F TS Series, Sealed (GY)

#### Connector Part Information

- OEM: 6188-0173
- Service: See catalog
- Description: 6-Way M TS 090 Series, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray:8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: Terminal Repair Kit
- Release Tool/Test Probe: Terminal Repair Kit

#### X407 Rear Chassis Harness to Right Rear Lamp Assembly Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 0.8 D-GN | 619 | Right Rear Turn Signal Lamp Supply Voltage | 2 | 0.8 GN | 619 | Right Rear Turn Signal Lamp Supply Voltage
3 | 0.8 WH | 609 | Right Tail Lamp Supply Voltage | 3 | 0.8 WH | 609 | Right Tail Lamp Supply Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 0.8 BK | 750 | Ground | 5 | 0.8 BK | 750 | Ground
6 | 0.8 L-BU | 20 | Stop Lamp Supply Voltage | 6 | 0.8 GN/WH | 20 | Stop Lamp Supply Voltage

### X408 Chassis Harness to I/P Body Harness

#### Connector Part Information

- OEM: E-5225-001
- Service: 88988066
- Description: 8-Way F Sealed (BK)

#### Connector Part Information

- OEM: E-5222-003
- Service: 88988067
- Description: 8-Way M (BU)

#### Terminal Part Information

- Pins: 6-8
- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 1-5
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 2-6, 8
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 1, 7
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X408 Chassis Harness to I/P Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 BK | 750 | Ground | 1 | 0.8 BK | 750 | Ground
2 | 0.8 TN | 884 | Left Rear Wheel Speed Sensor Signal | 2 | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal
3 | 0.8 OG | 885 | Low Reference | 3 | 0.5 OG | 885 | Low Reference
4 | 0.8 BN | 882 | Right Rear Wheel Speed Sensor Signal | 4 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
5 | 0.8 WH | 883 | Low Reference | 5 | 0.5 WH | 883 | Low Reference
6 | 0.8 YE | 618 | Left Rear Stop/Turn Lamp Supply Voltage | 6 | 0.8 YE | 618 | Left Rear Stop/Turn Lamp Supply Voltage
7 | 0.8 D-BU | 809 | Left Tail Lamp Supply Voltage | 7 | 0.8 BK | 9 | Park Lamp Supply Voltage
8 | 0.8 D-GN | 619 | Right Rear Stop/Turn Lamp Supply Voltage | 8 | 0.8 D-GN | 619 | Right Rear Stop/Turn Lamp Supply Voltage

### X409 Chassis Harness to I/P Body Harness

#### Connector Part Information

- OEM: E-5092-001
- Service: 88988066
- Description: 1-Way F Sealed (BK)

#### Connector Part Information

- OEM: E-5096-001
- Service: 88988067
- Description: 1-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: See terminal Repair Kit
- Core/Insulation Crimp: See terminal Repair Kit
- Release Tool/Test Probe: See terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See terminal Repair Kit
- Core/Insulation Crimp: See terminal Repair Kit
- Release Tool/Test Probe: See terminal Repair Kit

#### X409 Chassis Harness to I/P Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 WH | 609 | Right Tail Lamp Supply Voltage | 1 | 0.8 BK | 9 | Park Lamp Supply Voltage

### X410 I/P Body Harness to the Rear Lamp Jumper Harness

#### Connector Part Information

- OEM: E-5651-1
- Service: See Catalog
- Description: 6-Way F Sealed (BK)

#### Connector Part Information

- OEM: E-5655-2
- Service: See Catalog
- Description: 6-Way M Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See terminal Repair Kit
- Core/Insulation Crimp: See terminal Repair Kit
- Release Tool/Test Probe: See terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See terminal Repair Kit
- Core/Insulation Crimp: See terminal Repair Kit
- Release Tool/Test Probe: See terminal Repair Kit

#### X410 I/P Body Harness to the Rear Lamp Jumper Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 BK | 750 | Ground | 1 | 0.8 BK | 750 | Ground
2 | 0.5 BN | 9 | Park Lamp Supply Voltage | 2 | 0.5 BN | 9 | Park Lamp Supply Voltage
3 | 0.8 L-GN | 24 | Ground | 3 | 0.5 L-GN | 24 | Ground
4 | 0.8 L-BU | 20 | Stop Lamp Supply Voltage | 4 | 0.5 L-BU | 20 | Stop Lamp Supply Voltage
5 | 0.5 OG | 122 | Rear Fog Lamp Supply Voltage | 5 | 0.5 OG | 122 | Rear Fog Lamp Supply Voltage
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

### X500 Driver Door Harness to the I/P Body Harness

#### Connector Part Information

- OEM: 15326842
- Service: See Catalog
- Description: 10-Way F 150 Sealed (BK)

#### Connector Part Information

- OEM: 15326847
- Service: See Catalog
- Description: 10-Way M 150 Sealed (BK)

#### Terminal Part Information

- Pins: A, B, C, D, E, F, G, H, J, K
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: A, B : 2/A
- Core/Insulation Crimp: Pins: C, D, E, F, G, H, J, K : E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A, B, C, D, E, F, G, H, J, K
- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: Pins: A, B : E/1
- Core/Insulation Crimp: Pins: C, D, E, F, G, H, J, K : E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X500 Driver Door Harness to the I/P Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 GY | 118 | Left Front Speaker Output (-) | A | 0.8 GY | 118 | Left Front Speaker Output (-)
B | 0.8 TN | 201 | Left Front Speaker Output (+) | B | 0.8 TN | 201 | Left Front Speaker Output (+)
C | 0.5 GY | 295 | Door Lock Actuator Lock Control | C | 0.5 GY | 295 | Door Lock Actuator Lock Control
D | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control (AU3/AU0) | D | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control (AU3/AU0)
D | 0.5 BK | 550 | Ground (without AU3) | D | 0.5 BK | 550 | Ground (without AU3)
E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage | E | GY | 8 | Instrument Panel Lamp Supply Voltage
F | 0.35 OG/WH | 881 | Passenger Mirror Motor Left Control | F | 0.35 OG/WH | 881 | Passenger Mirror Motor Left Control
G | 0.35 PK/WH | 889 | Passenger Mirror Motor Left/Down Control | G | 0.35 PK/WH | 889 | Passenger Mirror Motor Left/Down Control
H | 0.35 TN/WH | 330 | Right Mirror Motor Supply Voltage | H | 0.35 TN/WH | 330 | Right Mirror Motor Supply Voltage
J | 0.35 RD/WH | 440 | Battery Positive Voltage | J | 0.35 RD/WH | 440 | Battery Positive Voltage
K | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal | K | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal

### X501 Driver Door Harness to the I/P Body Harness (A31)

#### Connector Part Information

- OEM: 15326654
- Service: 88986254
- Description: 8-Way F GT 280 Series Sealed 5.8 (BK)

#### Connector Part Information

- OEM: 15326655
- Service: 15306424
- Description: 8-Way M GT 280 Series Sealed 5.8 (BK)

#### Terminal Part Information

- Pins: A, B, C
- Terminal/Tray: 15304720/19
- Core/Insulation Crimp: 4/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: D
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A, B, C, D
- Terminal/Tray: 15304732/8
- Core/Insulation Crimp: A/5
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X501 Driver Door Harness to the I/P Body Harness (A31)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal | A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal
B | 2.0 BK | 550 | Ground | B | 2.0 BK | 550 | Ground
C | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage | C | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal | D | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal
E | 1.0 RD/WH | 240 | Battery Positive Voltage | E | 1.0 RD/WH | 240 | Battery Positive Voltage
F | 0.5 WH | 682 | Door Lock Lock/Unlock Signal | F | 0.35 WH | 682 | Door Lock Lock/Unlock Signal
G-H | -- | -- | Not Used | G-H | -- | -- | Not Used

### X505 Driver Door Harness to Power Mirror Switch Harness

#### Connector Part Information

- OEM: 15322158
- Service: See Catalog
- Description: 10-Way F 150 Sealed (BK)

#### Connector Part Information

- OEM: 15332153
- Service: See Catalog
- Description: 10-Way M 150 Sealed (BK)

#### Terminal Part Information

- Pins: A, B, C, D, E, F, G, H, J, K
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: A, B : 2/A
- Core/Insulation Crimp: Pins: C, D, E, F, G, H, J, K : E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A, B, C, D, E, F, G, H, J, K
- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: Pins: A, B : E/1
- Core/Insulation Crimp: Pins: C, D, E, F, G, H, J, K : E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X505 Driver Door Harness to Power Mirror Switch Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | 0.35 BK | 550 | Ground | B | 0.35 BK | 550 | Ground
C | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage | C | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage
D | 0.35 WH | 81 | Driver Mirror Motor Right Control | D | 0.35 WH | 81 | Driver Mirror Motor Right Control
E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage | E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
F | 0.35 L-GN | 89 | Driver Mirror Motor Down Control | F | 0.35 L-GN | 89 | Driver Mirror Motor Down Control
G | 0.35 RD/WH | 440 | Battery Positive Voltage | G | 0.35 RD/WH | 440 | Battery Positive Voltage
H | 0.35 TN | 329 | Driver Mirror Motor Supply Voltage | H | 0.35 TN | 329 | Driver Mirror Motor Supply Voltage
J | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control | J | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control
K | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control | K | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control

### X600 Passenger Door Harness to the Instrument Panel Body Harness

#### Connector Part Information

- OEM: 15326084
- Service: 15306348
- Description: 16-Way F GT 150 280 Series Sealed 4.0 5.8 (BK)

#### Connector Part Information

- OEM: 15326085
- Service: 15306122
- Description: 16-Way M GT 150 280 Series Sealed 4.0 5.8 (BK)

#### Terminal Part Information

- Pins: B, C, D, E, F, G, K, L, N, P
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: B, C : 2/A
- Core/Insulation Crimp: Pins: D, E, F, G, K, L, N, P : E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A, J, S
- Terminal/Tray: 15304720/19
- Core/Insulation Crimp: 4/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A, J, S
- Terminal/Tray: 15304732/8
- Core/Insulation Crimp: A/5
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: B, C, D, E, F, G, K, L, N, P
- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: Pins: B, C : E/1
- Core/Insulation Crimp: Pins: D, E, F, G, K, L, N, P : E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X600 Passenger Door Harness to the Instrument Panel Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal | A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal
B | 0.8 D-GN | 117 | Right Front Speaker Output (-) | B | 0.8 D-GN | 117 | Right Front Speaker Output (-)
C | 0.8 L-GN | 200 | Right Front Speaker Output (+) | C | 0.8 L-GN | 200 | Right Front Speaker Output (+)
D | 0.5 TN | 294 | Door Lock Actuator Unlock Control | D | 0.5 TN | 294 | Door Lock Actuator Unlock Control
E | 0.5 GY | 295 | Door Lock Actuator Lock Control | E | 0.5 GY | 295 | Door Lock Actuator Lock Control
F | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage | F | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
G | 0.35 GY | 881 | Passenger Mirror Motor Left Control | G | 0.35 GY | 881 | Passenger Mirror Motor Left Control
H | -- | -- | Not Used | H | -- | -- | Not Used
J | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage | J | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
K | 0.35 BN/WH | 889 | Passenger Mirror Motor Left/Down Control | K | 0.35 BN/WH | 889 | Passenger Mirror Motor Left/Down Control
L | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage | L | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage
M | 0.5 WH | 682 | Door Lock Lock/Unlock Signal | M | 0.5 WH | 682 | Door Lock Lock/Unlock Signal
N | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal | N | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal
P | 0.35 BK | 550 | Ground | P | 0.35 BK | 550 | Ground
R | -- | -- | Not Used | R | -- | -- | Not Used
S | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal | S | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal