For 1990-2009 cars

### Removal Procedure

1. Remove the right engine mount. Refer to Engine Mount Replacement - Right Side.
2. Remove the engine mount bracket bolts and bracket.

### Installation Procedure

1. Position the right engine mount bracket to the engine block.
2. Install the engine mount bracket bolts until snug.

Caution: Refer to Fastener Caution in the Preface section.

3. Tighten the right engine mount bracket bolts in the following sequence, to 55 N·m (41 lb ft).

3.1. | Lower rear

3.2. | Upper front

3.3. | Lower front

3.4. | Upper rear

4. Install the right engine mount. Refer to Engine Mount Replacement - Right Side.