For 1990-2009 cars

# Convertible Top Material Pinching at Rear Weatherstrip When Closing (Apply Weatherstrip Lubricant or Dielectric Silicone Grease to Weatherstrip)

Subject: | Convertible Top Material Pinching at Rear Weatherstrip When Closing (Apply Weatherstrip Lubricant or Dielectric Silicone Grease to Weatherstrip)

Models: | 2006-2009 Pontiac Solstice

| 2007-2009 Saturn SKY

| 2007-2009 Opel GT

| 2007-2008 Daewoo G2X

### Condition

Some customers may comment that when they put the convertible top up, they notice the top material becomes pinched in the area of the center of the door glass.

### Correction

Cover the front seats and apply a liberal coating of dielectric silicone grease to the area shown in the illustration above.

### Parts Information

Each tub of dielectric silicone grease will service approximately 10 vehicles.

Part Number | Description | Material Allowance
--- | --- | ---
12345579 (US) | Dielectric Silicone Grease | $0.93 per vehicle (US) $0.75 per vehicle (Canada)
10953481 (Canada)

### Warranty Information

For vehicle repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
B9858* | Apply Weatherstrip Lubricant | 0.2 hr
*This is a unique labor operation for bulletin use only. It will not be published in the Labor Time Guide.