For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Driver and Passenger Seat Replacement .
2. Remove the front seat back cushion cover and pad. Refer to Seat Back Cover and Pad Replacement .

1 | Seat Recliner Handle Tip Pull the handle away from the seat to remove.
2 | Seat Recliner Outer Cover Tip Unclip the rear of the cover first then slide away from seat to remove.
3 | Seat Back Cushion Frame Retainer Clip (Qty: 2)
4 | Seat Back Cushion Frame Assembly

#### Procedure

1. Tilt the seat back forward.
2. Pull the front part of the frame away from the pivot studs to remove.