For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the forward portion of the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .
3. Disconnect the fog lamp bulb socket electrical connector.

1 | Front Fog Lamp Assembly Screw (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Fog Lamp Assembly Procedure Remove the lamp assembly from the fog lamp bracket.
3 | Front Fog Lamp Bulb Caution: Refer to Halogen Bulb Caution in the Preface section. Tip Turn the bulb socket counterclockwise and remove from the fog lamp assembly.
4 | Adjuster Screw

#### Procedure

1. Remove the screw in order to separate the fog lamp from the fog lamp ring.
2. Aim the fog lamps after replacement of the fog lamp assembly. Refer to Fog Lamp Aiming .