For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Shift Indicator

#### Procedure

1. Grasp the edge of the shift indicator bezel by reaching under the bezel from the soft boot area. Lift the shift indicator bezel up to release the bezel from the instrument panel cluster trim plate.
2. Disconnect the shift indicator electrical connector.

2 | Shift Control Range Select Lever Clip Tip Do not reuse the clip.
3 | Shift Control Knob Retaining Screw Caution: Refer to Fastener Caution in the Preface section. Tip Loosen the screw 3 turns. It is not necessary to fully remove the screw in order to remove the shift control knob from the shift control lever. Tighten
2.5 N·m (22 lb in)

4 | Shift Control Knob