For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.
3. Disengage the connector positive assurance (CPA) clip from the wiper motor electrical connector.
4. Disconnect the wiper motor electrical connector from the wiper motor.

1 | Windshield Washer System Module Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Procedure

1. Install the driver side bolt first.
2. Install the passenger side bolt second.
3. Install the center bolt third.

Tighten
10 N·m (89 lb in)

2 | Windshield Washer System Module Assembly