For 1990-2009 cars

### Removal Procedure

1. Remove the charge air cooler inlet pipe. Refer to Charge Air Cooler Inlet Pipe Replacement.
2. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement.
3. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.
4. Disconnect the engine wiring harness electrical connector (1) from the mass air flow (MAF) sensor.
5. Remove the air cleaner assembly front bolt.
6. Firmly tug on the air cleaner lower assembly in order to disengage the air cleaner from the studs.
7. Remove the air cleaner assembly from the vehicle.

### Installation Procedure

1. Install the air cleaner assembly to the vehicle.
2. Position the air cleaner assembly over the studs. Firmly press down over the studs in order to engage the air cleaner to the studs.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the air cleaner assembly front bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Connect the engine wiring harness electrical connector (1) to the MAF sensor.
5. Install the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.
6. Install the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement.
7. Install the charge air cooler inlet pipe. Refer to Charge Air Cooler Inlet Pipe Replacement.