For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise the vehicle. Refer to Lifting and Jacking the Vehicle .

1 | Stabilizer Shaft Mounting Bracket Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tip The bolts DO NOT have to be removed for this procedure. Loosen the bolts until the insulator can be removed from the stabilizer shaft. Tighten
55 N·m (41 lb ft)

2 | Stabilizer Shaft Mounting Bracket
3 | Stabilizer Shaft Insulator