For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Reach in behind the heat shield material located on the rear bumper filler panel extension in order to access the back up lamp bulbs.
2. Reach under the rear bumper filler heat shield material and twist the upper lamp socket counterclockwise.

1 | Electrical Harness Connector
2 | Backup Lamp Assembly Socket Tip Rotate the socket counterclockwise and remove from the lamp housing.
3 | Backup Lamp Assembly Bulb Tip Pull the bulb straight from the lamp socket in order to remove.