For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Drain only the fluid from the radiator surge tank. Refer to Cooling System Draining and Filling.

1 | Radiator Surge Tank Cap Assembly
2 | Radiator Surge Tank Retainer
3 | Radiator Surge Tank Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
4 | Radiator Surge Tank Assembly

#### Procedure

Using J 38185 , position radiator surge tank hose clamps aside and remove hoses from the radiator surge tank.

#### Special Tools

J 38185 Hose Clamp Pliers