For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the interior trim panel. Refer to Door Trim Panel Replacement .

1 | Outside Door Handle Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

1. Pull the upper corner of the water deflector down to access the outside handle bolts.
2. Release the lock rod from the lock cylinder.

Tighten
10 N·m (89 lb in)

2 | Front Door Outside Handle