For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the drive flange and seal. Refer to Drive Flange and Seal Replacement.

1 | Extension Housing Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Extension Housing
3 | Extension Housing Seal Tip The extension housing seal is reusable. Replace the seal ONLY if the sealing surface is no longer in usable condition.