For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Brake Dust Caution in the Preface section. Notice: Support the brake caliper with heavy mechanic wire, or equivalent, whenever it is separated from its mount and the hydraulic flexible brake hose is still connected. Failure to support the caliper in this manner will cause the flexible brake hose to bear the weight of the caliper, which may cause damage to the brake hose and in turn may cause a brake fluid leak.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation .

1 | Rear Disc Brake Caliper Guide Pin Seal (Qty: 2)
2 | Rear Disc Brake Caliper Guide Pin Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 27 N·m (20 lb ft)
3 | Rear Disc Brake Caliper
4 | Rear Disc Brake Caliper Guide Pin Bushing (Qty: 2)
5 | Rear Disc Brake Caliper Spring

#### Procedure

Thoroughly clean the brake pad hardware mating surfaces of the brake caliper bracket of any debris or corrosion. If excessive corrosion exists, replace the brake caliper bracket. Refer to Rear Brake Caliper Bracket Replacement .