For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Differential Mounting Bracket to Frame Bolt Caution: Refer to Fastener Caution in the Preface section. Tip

• | Use a jack stand to support the differential.

• | The bracket service part is supplied with a pre-installed dowel pin. Remove the pin if there is no corresponding hole in the axle housing bracket mounting surface.

Tighten
175 N·m (124 lb ft)

2 | Differential to Mounting Bracket Bolt Tighten

• | 250 N·m (184 lb ft) for mounting bracket with dowel pin

• | 350 N·m (258 lb ft) for mounting bracket without dowel pin

3 | Differential Mounting Bracket