For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front floor console. Refer to Front Floor Console Replacement .
2. With the park brake lever fully released, completely back off the cable adjustment nut.

The park brake cable adjusting nut is a nylon lock type. Use ONLY HAND TOOLS whenever tightening or loosening the adjusting nut.

3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .

1 | Front Park Brake Cable

#### Procedure

1. Carefully position the driveline tunnel insulator downward just enough to access the cable equalizer.
2. Rotate the front cable end to release the cable from the equalizer.

2 | Park Brake Lever Nut (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
3 | Park Brake Lever Assembly

#### Procedure

1. Disconnect the electrical connector from the park brake warning lamp switch.
2. Adjust the tension of the park brake cables. Refer to Park Brake Adjustment .