For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear muffler assembly. Refer to Muffler Replacement .
3. Remove the stabilizer shaft links from the end of the stabilizer shaft. Refer to Stabilizer Shaft Link Replacement .

Important: If removing the stabilizer shaft to service other suspension components, it is not necessary to remove the stabilizer shaft insulators.

4. Remove the stabilizer shaft brackets. Refer to Stabilizer Shaft Insulator Replacement .
5. Remove the right lower shock module bolts to the lower control arm. Refer to Shock Absorber and Spring Assembly Replacement .
6. Remove the rear stabilizer shaft from the vehicle.

### Installation Procedure

1. Position the stabilizer shaft in the vehicle.
2. Install the stabilizer shaft brackets. Refer to Stabilizer Shaft Insulator Replacement .
3. Install the stabilizer shaft links to the end of the stabilizer shaft. Refer to Stabilizer Shaft Link Replacement .
4. Install the right lower shock module bolts to the lower control arm. Refer to Shock Absorber and Spring Assembly Replacement .
5. Install the rear muffler assembly. Refer to Muffler Replacement .
6. Lower the vehicle. Refer to Lifting and Jacking the Vehicle .