For 1990-2009 cars

Application | Front Runout | Center Runout | Rear Runout | Stub Shaft Runout
--- | --- | --- | --- | ---
Metric | English | Metric | English | Metric | English | Metric | English
1 Piece Propeller Shaft - Guideline | 1.17 mm | 0.046 in | 1.27 mm | 0.050 in | 1.40 mm | 0.055 in | -- | --
1 Piece Aluminum Graphite Propeller Shaft - Guideline | 1.17 mm | 0.046 in | -- | -- | 1.40 mm | 0.055 in | -- | --
2 Piece System Front Propeller Shaft with Slip Yoke - Guideline | 0.76 mm | 0.030 in | 0.76 mm | 0.030 in | 0.71 mm | 0.028 in | -- | --
2 Piece System Front Propeller Shaft with Stub Shaft - Guideline | 0.76 mm | 0.030 in | 0.76 mm | 0.030 in | -- | -- | 0.13 mm | 0.005 in
2 Piece System Rear Propeller Shaft with Slip Yoke - Guideline | 0.71 mm | 0.028 in | 0.76 mm | 0.030 in | 0.89 mm | 0.035 in | -- | --
2 Piece System Rear Propeller Shaft with Stub Shaft - Guideline | -- | -- | 0.76 mm | 0.030 in | 0.89 mm | 0.035 in | 0.13 mm | 0.005 in
These guidelines apply only to propeller systems with 2 or 3 U-joints.