For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Rear Compartment Lid Hold-Open Device Caution in the Preface section.

#### Preliminary Procedure

Remove the rear fascia. Refer to Rear Bumper Fascia Replacement .

1 | Rear Compartment Lid Torque Rods Tip

1. Use tool J 39384-10 Torsion Rod Adjustment Bar.
2. Install torque rods with rear compartment lid closed.
3. Engage the ends of the torque rods into the cam link.
4. Open deck lid and engage the fixed end into the hinges.