For 1990-2009 cars

### Removal Procedure

1. Remove the fuel feed intermediate pipe. Refer to Fuel Feed Intermediate Pipe Replacement .
2. Disconnect the engine wiring harness electrical connector (2) from the intake camshaft position (CMP) sensor.
3. Remove the CMP sensor bolt.
4. Remove the CMP sensor.

### Installation Procedure

Important: Inspect the CMP sensor for damage, replace as necessary.

1. Lubricate the CMP sensor O-ring seal with clean engine oil.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CMP sensor.
3. Install the CMP sensor bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Connect the engine wiring harness electrical connector (2) to the intake CMP sensor.
5. Install the fuel feed intermediate pipe. Refer to Fuel Feed Intermediate Pipe Replacement .