For 1990-2009 cars

### Removal Procedure

1. Remove the turbocharger. Refer to Turbocharger Replacement.
2. Remove the turbocharger oil return hose bolts (2) and hose from the turbocharger.
3. Remove and discard the turbocharger oil return hose gasket (1).

### Installation Procedure

1. Lubricate and install a NEW turbocharger oil return hose O-ring seal (3).
2. Position a NEW turbocharger oil return hose gasket (1) on the turbocharger oil return hose.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the turbocharger oil return hose and bolts (2).

Tighten the bolts to 10 N·m (89 lb in).

4. Install the turbocharger. Refer to Turbocharger Replacement.