For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front floor closeout panel. Refer to Floor Panel Tunnel Panel Replacement - Front .
3. Remove the floor panel tunnel rear panel. Refer to Floor Panel Tunnel Panel Replacement - Rear .
4. Support the transmission.
5. Remove the transmission support. Refer to Transmission Support Replacement .

1 | Transmission Mount Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 55 N·m (41 lb ft)
2 | Transmission Mount
3 | Transmission Mount Adaptor Bolt (Qty: 4) Tighten 55 N·m (41 lb ft)
4 | Transmission Mount Adaptor