For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlamps. Refer to Headlamp Replacement.

1 | Hood Hinge Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tip

1. Disconnect the wiring harness from the hood on both sides.
2. Mark the hood for proper alignment for re-installing.

Tighten
25 N·m (18 lb ft)

2 | Hood Warning: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.