For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the outside door handle. Refer to Door Outside Handle Replacement .

1 | Lock Cylinder Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Side Door Outside Handle Lock Cylinder